## Keyboard shortcuts

Press `←` or `→` to navigate between chapters

Press `S` or `/` to search in the book

Press `?` to show this help

Press `Esc` to hide this help

# Data access pattern

In the `UserMatCPU`, arrays with the `p_` prefix are data pointers to arrays used for calculation of material response.

Since arrays are structured per integration point for CPU implementation, there is no need to calculate global offsets. For instance, `p_strain[0]` through `p_strain[5]` relate to the current integration point.